Installation NOTES FOR MS-WINDOWS 7/10 PRO:

ATTENTION: If UPDATING software, please uninstall any older version
of the PTC USBXpress driver. All old driver files must be removed 
from the computer drive. An old main library file SiUSBXp.DLL must
be removed; it is usually located in the application directory for the PTC.

1. Install the PTC USBXpress driver for MS Windows 7/10 PRO:
- Determine the processor type for your computer: x64 (most) or x86 (older type)
- Run corresponding USBXpressInstaller_x64/_x86 files in Drivers folder
- Check (in the Application Directory for the PTC) for the SiUSBXp.DLL file
  (ver. 3.12.0.0 or later); if needed, copy it there from this folder.

2. Optional - ONLY for micrometers that use USB GaugeWay Interface Device for 
       	     continuous reading: 
- run the MitutoyoUSBGaugeWay.exe program

3. Optional: Scale (Mass Balance) Serial-to-USB adapter:
- just plug in the cable - typically the driver installs automatically 
- if needed, select the Install option on the adapter-specific installation CD

NOTE-1: PC Administrator access is required !
NOTE-2: We currently use micrometer USB Adapter Cable that transfers readings by 
	pressing a button. There is no need for a dedicated driver. 